How to setup SAT and IPSec VPN on wan2

  IP:192.168.10.10/24

  WAN:10.10.10.2/24

 IP:10.10.10.1/24

IP:103.10.10.2/24

 

 WAN1:DHCP WAN2:103.10.10.1/24

  DFL-800

  

 IP:192.168.1.3/24 IP:192.168.1.200/24

 HTTP server FTP server

(1)Go to “Ethernet” to change IP address.



(2)Go to “Object” -> “Authentication objects”.Add a new pre-share key.



(3)Go to “Interface” -> “IPSec”. Add a new IPSec tunnel.



(4)Go to “main table”. Add a new route. Please be carefully “network” and “gateway”.



(5)Go to “Rule” -> “Access”. Add a new accept rule for wan2.



(6)Go to “Rule” -> “IP Rules”. Add two new rules for VPN.



(7)Go to “routing”. Add a new PBR table.



(8)Go to “routing” -> “routing rules”. Add a new rule for PBR table.



(9)Go to “Rule” -> “IP Rules”. Add four new rules for SAT.









