How to setup SIP ALG

 SIP Server: Public IP

Internet

WAN IP: PPPoE


DFL-800


SIP Phone: X-Lite 4.0 SIP Phone: X-Lite 4.0


This topology is reference “NetDefendOS\_2.27.03\_Firewall\_UserManual” P.273 scenario 1. You can study chapter 6.2.8. “The SIP ALG”. It can make you understand SIP ALG more detail.

1. Add a new SIP ALG.




1. Add a new SIP-UDP service.





1. Add two new IP rules “SIP” and “SIP-IN”.



1. Change timeout settings.

