The FW version later 2.40.00.10 support IPv6 Function.

In this KM, we will know how to enable IPv6 Router Advertisement function on DFL.

1. Go to System/Advanced Settings/IP Settings, click “Enable IPv6”.



1. And then enable the IPv6 on the interface.



1. On page “Advanced”, enable the router advertisement function.

