

**[Step]**


1.You can add the IP4 group(named DMZ\_LAN) which contains lannet and dmznet on Address Book.




2. And then add the interface group (named DMZ\_LAN) which contains LAN port and DMZ port on Interfaces.



3. Finally, the IP Rules has changed.





(DFL-860E firmware is 2.40.00.10-16817)

